Update Releases

03.29.2025 - Update

  1. Fixed Vivo Red State after FRP.
     
     *** Always Select "FRP New Security (2024, 2025) for newer Android 14 and 15 phones

  2. Added a more visible Location for the following information:
       Boot Partition
       Reference Clock
       Configuration Descriptor (OTP)
       Partition Setting Locked (eMMC)
 
  3. Added dLUNumWriteBoosterBufferAllocUnits in saving and writing UFS provision.xml
 
  4. Improved eMMC ISP Read Speed

  5. Improved Samsung FRP Remove


03.21.2025d - Quick Fix
   
  1. Fixed eMMC Qualcomm GPT file loading. (Thanks to SadaM)

03.21.2025 - New Features and Bug Fixes

  1. Added eMMC RPMB Set Counter to match previous RPMB Counter on Qualcomm Phones (Requested by Ramana)

  2. Fixed Samsung eMMC RPMB Size Change (Reported by Abdullah Rasheed)

  3. Fixed eMMC RPMB Read Counter Stuck on ISP

  4. Added automatic loading of Qualcomm gpt_main0.bin, gpt_main1.bin etc in partition list.
     * With automatic Repartition.

  5. Added Android Boot slot Change A/B 

  6. Remove Factory Reset Button in Partition List
     * Now you need to use Erase User Data and choose the proper option best suited for
       your phone. Do this AT YOUR OWN RISK.
 
  7. Added Samsung eMMC Firmwares
     CKTA42 : KLMCG2KCTA-B041
     CUTA42 : KLMCG2UCTA-B041
     DD68MB : KMDD60018M-B320
     DH6DAB : KMDH6001DA-B425
     DP6DBB : KMDP6001DB-B425
     DUTA42 : KLMDG4UCTA-B041
     DV6DBB : KMDV6001DB-B620
     DV6DMB : KMDV6001DM-B620
     DX68MB : KMDX60018M-B425
     FE62MB : KMFE60012M-B214
     GP6BMB : KMGP6001BM-B514
     GX6BAB : KMGX6001BA-B514
     QX63AB : KMQX60013A-B419
     QX63MB : KMQX60013M-B419

  8. Added SkHynix eMMC Fimrwares
     H8G4a2
     HAG4a2
     HCG8a4

  9. Fixed SGPT Generation for MTK and Qualcomm


02.27.2025 - End User Requests and Bug Fixes

  1. Added AI Connect (Autonomous Interaction)
     This feature will automatically reconnect if communication 
     errors are detected. This helps when connecting phones
     via ISP using USB power only (No Vcc and VccQ). The feature
     is enabled by default.

  2. Added support for malformed GPT Headers from some Moto Phones.

  3. Added EMMC Firmware Contributed by End User
     QE63MB : KMQE60013M-B318 (by s.l.m.)


02.24.2025 - End User Requests and Bug Fixes
  
  1. Fixed Erase of very small partition sizes

  2. Remove nag Screen "Please click Yes 3 times"

  3. Increased UFS Inactivity Timeout 


02.23.2025 - End User Requests and Bug Fixes
  
  1. Fixed GPT and SGPT Sizes for newer MTK based Soc

  2. Fixed FRP on older Androids - Thanks to KUMAR VISHWAKARMA

  3. Added EMMC Firmware Contributed by End User
     3V6CAB : KM3V6001CM-B708 (by Bilal Akash)


02.18.2025 - End User Requests and Bug Fixes

  1. Added New FRP Remove Option for persistent partition data fill
     * You can now select to fill partition with 0xFF or 0x00
  
  2. Added EMMC Firmware Contributed by End Users:
     3V6CBB : KM3V6001CM-B705 (by yu luosheng)

  3. UFS Amplitude Setting now defaults at 316 mV for more compatibility


02.15.2025 - End User Requests and Bug Fixes

  1. Initial support for Monitors with less than 1080p Resolution

  2. Added EMMC Firmware Contributed by End Users:
     RC14MB : KMRC10014M-B809 (by SadaM)
     BJTD4R : KLMBG2JETD-B041 (by SadaM)
     GX6BAB : KMGX6001BA-B514 (by SadaM)
     DV6DBB : KMDV6001DB-B625 (by SadaM)
     QD63MB : KMQD60013M-B318 (by SadaM)
     QX63AB : KMQX60013A-B419 (by SadaM)


02.14.2025 - End User Requests and Bug Fixes
  
  1. Fixed sboot target partition from PIT for the following Exynos SoC:
    * Reported by MasterUnlockGSM from Venezuela    
       Exynos 1280
       Exynos 1330
       Exynos 1380
       Exynos 1480
       Exynos 1580
       Exynos 2200
       Exynos 2400
    
    
  2. Added PIT File Support for UFS Provisioning

  3. Fixed MTK Preloader Boot Relay Table for newer SoCs (UFS and EMMC)     
    * Reported by Knotthailand

  4. Added SkHynix EMMC FFU files for:
       hB8aP>
       hC8aP>
       hC9aP3
       hDEaP3

    * These eMMC Firmware will allow RPMB Key Reading, Unlimited Repartitioning, WP Removal and CID/CSD Write
    * Performing FFU on SK Hynix eMMC will NOT result in data loss.
    * Avoid performing multiple FFU operations on the same eMMC, as its firmware uses a static NAND page address. 
      This means the page cannot be relocated if bad blocks begin to develop.

  5. Added the ability to set the working directory using the HOME button located at the lower right corner of the software.
     * Suggested by MasterUnlockGSM from Venezuela

  6. A separate rawprogram.xml per LUN will now be generated during partition backups.
     * Suggested by MasterUnlockGSM from Venezuela

  7. Enhanced the speed of FFU reading for Samsung eMMC.

  8. UFS VCC is now set to 2.80V by default.

  9. Added support for UFS 4.1 new descriptors, attributes and flags.


02.05.2025 - End User Requests and Bug Fixes

  1. Added eMMC Boot Config Information in Connection Logs

  2. Added Auto LBA Skip on eMMC with Secure Write Protected Blocks

  3. Added Detailed Connection ERROR Resolution for UFS ISP

  4. Added EMMC Firmware Contributed by End Users:
     DV6DAB : KMDV6001DA-B620 (By Knotthailand)
     GD6BMB : KMGD6001BM-B421 (By Knotthailand)
     DC6DMB : KMDC6001DM-B625 (By Knotthailand)

  5. Fixed GUI Freeze on UFS and EMMC Read Timeouts


02.01.2025 - Initial Update and Bug Fixes
  
  1. Added Auto LBA Skip on UFS with Secure Write Protected Blocks

  2. Added UFS Secure Write Protection Removal (WP Remove)

     ** Use this option at your own risk **

     According to our tests, most UFS will suffer 100% Data Loss with
     a very few exception listed below
     
     Brand  | UFS Specification | Data Status after WP Remove
    -------------------------------------------------------------
    Samsung | 2.0               | NO Data Loss
    Samsung | 2.1               | NO Data Loss
    Samsung | 2.2               | NO Data Loss
    Samsung | 3.0               | NO Data Loss
    Samsung | 3.1               | NO Data Loss
    Samsung | 4.0               | WARNING 100% Data Loss on all LUNs !!! - make backup all LUNs !!!
    -------------------------------------------------------------
    YMTC    | 2.2               | NO Data Loss
    -------------------------------------------------------------
    Other Brands (SkHynix, Micron, KIOXIA etc...) will experience 100% Data Loss on all LUNs !!! - make backup all LUNs !!!


01.22.2025 - Initial Early Release







Official Releases

  NONE
     


             