Update Releases

06.02.2025 - Update
  
  1. Added Support for Xioami Xring O1 Devices (Xiaomi 15S Pro, Xioami Pad 7 Ulta, etc)
     * UFS Provisioning supported via gpt.img (Xioami GPT File)
     * Full Firmware Flashing supported via flash.bat / flash.sh
     * Full Firmware Flashing supported via fdt_sec.xml (Xioami XML File)   

  2. Added Support for SPD/Unisoc FileList.ini Flashing using Official Firmware

  3. Added Motorola UTAG partition parsing (Thanks to Mr.UPROM)

  4. Added SKU to Phone Model matching for Samsung, Vivo, Realme, Oppo, Nubia and Xiaomi_models

  5. Added skip Userdata option for RAW Partition Reading (Thanks to Mr.UPROM)

  6. Added quick access to eMMC Boot Configuration in Partition Tab (Thanks to yu luosheng)

  7. Fixed Exynos impoper parsing of partitions inside SUPER (Thanks to Giovanni Lucas Da Paz)

  8. Improved "AI Connect" for eMMC ISP Flashing Sparsed Files (Thanks to hello-firmware.com)

  9. Improved eMMC Erase Function

 10. Improved COMBO_BOOT detection on MTK Preloaders (Thanks to hello-firmware.com)

 11. Added New Samsung FFU:
     GP6BAB : KMGP6001BA-B514 (by 0x9k)
     CUTB42 : KLMCG2UCTB-B041 (by hello-firmware.com)
     GX6BMB : KMGX6001BM-B514
     RD64MB : KMRD60014M-B512
     RH64AB : KMRH60014A-B614
     RE1BMB : KMRE1000BM-B512
     RC1BMB : KMRC1000BM-B809
     FE12MB : KMFE10012M-B214
     BWBD3R : KLMBG4WEBD-B031


05.19.2025 - Update

  1. Fixed a MAJOR erase bug on small eMMC partitions (Thanks to hello-firmware.com).

  2. Added MTK Direct Preloader Header Generation for manually loaded files (Thanks to hello-firmware.com).

  3. Improved Android Security automatic backup file saving (Thanks to Giovanni Lucas Da Paz).

  4. Improved rawprogram.xml universal backup file format (Thanks to Master Unlock GSM).

  5. Moved BOOT A and BOOT B eMMC partitions to the top (Thanks to sohrab ezi).

  6. Fixed BOOT A and BOOT B raw partition writing (Thanks to sohrab ezi).

  7. Fixed Unisoc SPL loader flashing for Samsung factory files (Thanks to Nguyễn Diện and Giovanni Lucas Da Paz).

  8. Added "Backup Security" button** in the Partitions tab.

  9. Moved "Erase Before Write" option in the Partitions tab.

 10. Added "Fake" Health Repair firmwares for SK Hynix hB8aP>, hC8aP>, hC9aP3, and hDEaP3

    * These FFU firmwares do not repair health, but only make the eMMC report that its health is "Perfect."
    * These FFU firmwares have "\_HR" at the end of the filename, e.g., 30_HYNIX_hB8aP__0060_PATCHED_FINAL_HR.fw.
 
 11. Samsung eMMC FFU Filename now includes the IC Marking (Thanks to sohrab ezi).

 12. Added New Samsung FFU:
     QE13MB : KMQE10013M-B318 (by 0x9k)
     QX63AB : KMQX60013A-B419 (by 0x9k)
     MCG8GC : KLMCG8GEAC-B001
     DH6DMB : KMDH6001DM-B422
     RX14MB : KMRX10014M-B614
     QX13MB : KMQX10013M-B419
     RX1BMB : KMRX1000BM-B614
     RX64MB : KMRX60014M-B614

 13. Improved MTK Preloader IC Check for supported UFS / EMMC check

 14. Added MBR/GPT repartition support for Phones that does not use BackupGPT (Kirin based) (Thanks to Mr.UPROM).

 15. Fixed UFS Provisioning of LU Dedicated WriteBooster (Thanks to Giovanni Lucas Da Paz). 

 
04.30.2025 - Update

  1. Fixed Android Info Reading for Motorola Phones

  2. Fixed Boot Mode eMMC FFU to not change CID

  3. Fixed Micron UFS Provision Bug

  4. Added UFS Erase all LUNS Button
     * Use this to fix "slow" UFS IC
     * This is a safer option than Provisioning the UFS
     * Does not require OTP Unlock
     * Does not Erase RPMB Data
     * Does not Erase Write Protected Areas

  5. Added eMMC Erase All Partitions Button
     * Use this to Erase all Data from the eMMC
     * Resets eMMC BOOT Config
     * Does not Erase RPMB Data 

  6. Added Samsung eMMC Firmwares
     DUTB42 : KLMDG4UCTB-B041
     3H6CAB : KM3H6001CA-B515 
     DP68MB : KMDP60018M-B425 (by 0x9k)
     DV6DAB : KMDV6001DA-B620 (by 0x9k)

  7. Added Generic Android OEM Unlock
     * Additional Steps may be required to
       fully unlock the bootloader of the phone
       depending on the phone brand/manufacturer
 
  8. Added RPMB Write for UFS

  9. Improved Read/Backup Partition file (rawprogram.xml)
  
 10. Added EXT_CSD as part of eMMC Partition List

 11. Added Primary GPT and Backup GPT Check upon IC Detection (Thanks to KHUMAR ALOK VISHWAKARMA)

 12. Improved GPT Generation for Dimensity and Qualcomm UFS and eMMC (Thanks to Mr.)

 13. Automatic Boot Slot Selection when using flash_all.bat mi Factory Firmwares   

 14. Added Adjustable EMMC VCC On delay via Settings.ini EmmcVccInitDelay=2000 Entry
     * This value is in milliseconds
     * Adjustable from 40 upto 8000 milliseconds


03.29.2025 - Update

  1. Fixed Vivo Red State after FRP.
     
     *** Always Select "FRP New Security (2024, 2025) for newer Android 14 and 15 phones

  2. Added a more visible Location for the following information:
       Boot Partition
       Reference Clock
       Configuration Descriptor (OTP)
       Partition Setting Locked (eMMC)
 
  3. Added dLUNumWriteBoosterBufferAllocUnits in saving and writing UFS provision.xml
 
  4. Improved eMMC ISP Read Speed

  5. Improved Samsung FRP Remove


03.21.2025d - Quick Fix
   
  1. Fixed eMMC Qualcomm GPT file loading. (Thanks to SadaM)

03.21.2025 - New Features and Bug Fixes

  1. Added eMMC RPMB Set Counter to match previous RPMB Counter on Qualcomm Phones (Requested by Ramana)

  2. Fixed Samsung eMMC RPMB Size Change (Reported by Abdullah Rasheed)

  3. Fixed eMMC RPMB Read Counter Stuck on ISP

  4. Added automatic loading of Qualcomm gpt_main0.bin, gpt_main1.bin etc in partition list.
     * With automatic Repartition.

  5. Added Android Boot slot Change A/B 

  6. Remove Factory Reset Button in Partition List
     * Now you need to use Erase User Data and choose the proper option best suited for
       your phone. Do this AT YOUR OWN RISK.
 
  7. Added Samsung eMMC Firmwares
     CKTA42 : KLMCG2KCTA-B041
     CUTA42 : KLMCG2UCTA-B041
     DD68MB : KMDD60018M-B320
     DH6DAB : KMDH6001DA-B425
     DP6DBB : KMDP6001DB-B425
     DUTA42 : KLMDG4UCTA-B041
     DV6DBB : KMDV6001DB-B620
     DV6DMB : KMDV6001DM-B620
     DX68MB : KMDX60018M-B425
     FE62MB : KMFE60012M-B214
     GP6BMB : KMGP6001BM-B514
     GX6BAB : KMGX6001BA-B514
     QX63AB : KMQX60013A-B419
     QX63MB : KMQX60013M-B419

  8. Added SkHynix eMMC Fimrwares
     H8G4a2
     HAG4a2
     HCG8a4

  9. Fixed SGPT Generation for MTK and Qualcomm


02.27.2025 - End User Requests and Bug Fixes

  1. Added AI Connect (Autonomous Interaction)
     This feature will automatically reconnect if communication 
     errors are detected. This helps when connecting phones
     via ISP using USB power only (No Vcc and VccQ). The feature
     is enabled by default.

  2. Added support for malformed GPT Headers from some Moto Phones.

  3. Added EMMC Firmware Contributed by End User
     QE63MB : KMQE60013M-B318 (by s.l.m.)


02.24.2025 - End User Requests and Bug Fixes
  
  1. Fixed Erase of very small partition sizes

  2. Remove nag Screen "Please click Yes 3 times"

  3. Increased UFS Inactivity Timeout 


02.23.2025 - End User Requests and Bug Fixes
  
  1. Fixed GPT and SGPT Sizes for newer MTK based Soc

  2. Fixed FRP on older Androids - Thanks to KUMAR VISHWAKARMA

  3. Added EMMC Firmware Contributed by End User
     3V6CAB : KM3V6001CM-B708 (by Bilal Akash)


02.18.2025 - End User Requests and Bug Fixes

  1. Added New FRP Remove Option for persistent partition data fill
     * You can now select to fill partition with 0xFF or 0x00
  
  2. Added EMMC Firmware Contributed by End Users:
     3V6CBB : KM3V6001CM-B705 (by yu luosheng)

  3. UFS Amplitude Setting now defaults at 316 mV for more compatibility


02.15.2025 - End User Requests and Bug Fixes

  1. Initial support for Monitors with less than 1080p Resolution

  2. Added EMMC Firmware Contributed by End Users:
     RC14MB : KMRC10014M-B809 (by SadaM)
     BJTD4R : KLMBG2JETD-B041 (by SadaM)
     GX6BAB : KMGX6001BA-B514 (by SadaM)
     DV6DBB : KMDV6001DB-B625 (by SadaM)
     QD63MB : KMQD60013M-B318 (by SadaM)
     QX63AB : KMQX60013A-B419 (by SadaM)


02.14.2025 - End User Requests and Bug Fixes
  
  1. Fixed sboot target partition from PIT for the following Exynos SoC:
    * Reported by MasterUnlockGSM from Venezuela    
       Exynos 1280
       Exynos 1330
       Exynos 1380
       Exynos 1480
       Exynos 1580
       Exynos 2200
       Exynos 2400
    
    
  2. Added PIT File Support for UFS Provisioning

  3. Fixed MTK Preloader Boot Relay Table for newer SoCs (UFS and EMMC)     
    * Reported by Knotthailand

  4. Added SkHynix EMMC FFU files for:
       hB8aP>
       hC8aP>
       hC9aP3
       hDEaP3

    * These eMMC Firmware will allow RPMB Key Reading, Unlimited Repartitioning, WP Removal and CID/CSD Write
    * Performing FFU on SK Hynix eMMC will NOT result in data loss.
    * Avoid performing multiple FFU operations on the same eMMC, as its firmware uses a static NAND page address. 
      This means the page cannot be relocated if bad blocks begin to develop.

  5. Added the ability to set the working directory using the HOME button located at the lower right corner of the software.
     * Suggested by MasterUnlockGSM from Venezuela

  6. A separate rawprogram.xml per LUN will now be generated during partition backups.
     * Suggested by MasterUnlockGSM from Venezuela

  7. Enhanced the speed of FFU reading for Samsung eMMC.

  8. UFS VCC is now set to 2.80V by default.

  9. Added support for UFS 4.1 new descriptors, attributes and flags.


02.05.2025 - End User Requests and Bug Fixes

  1. Added eMMC Boot Config Information in Connection Logs

  2. Added Auto LBA Skip on eMMC with Secure Write Protected Blocks

  3. Added Detailed Connection ERROR Resolution for UFS ISP

  4. Added EMMC Firmware Contributed by End Users:
     DV6DAB : KMDV6001DA-B620 (By Knotthailand)
     GD6BMB : KMGD6001BM-B421 (By Knotthailand)
     DC6DMB : KMDC6001DM-B625 (By Knotthailand)

  5. Fixed GUI Freeze on UFS and EMMC Read Timeouts


02.01.2025 - Initial Update and Bug Fixes
  
  1. Added Auto LBA Skip on UFS with Secure Write Protected Blocks

  2. Added UFS Secure Write Protection Removal (WP Remove)

     ** Use this option at your own risk **

     According to our tests, most UFS will suffer 100% Data Loss with
     a very few exception listed below
     
     Brand  | UFS Specification | Data Status after WP Remove
    -------------------------------------------------------------
    Samsung | 2.0               | NO Data Loss
    Samsung | 2.1               | NO Data Loss
    Samsung | 2.2               | NO Data Loss
    Samsung | 3.0               | NO Data Loss
    Samsung | 3.1               | NO Data Loss
    Samsung | 4.0               | WARNING 100% Data Loss on all LUNs !!! - make backup all LUNs !!!
    -------------------------------------------------------------
    YMTC    | 2.2               | NO Data Loss
    -------------------------------------------------------------
    Other Brands (SkHynix, Micron, KIOXIA etc...) will experience 100% Data Loss on all LUNs !!! - make backup all LUNs !!!


01.22.2025 - Initial Early Release







Official Releases

  NONE
     


             